Hi everyone

I had some questions about assignment 12. The motor speeds are given in RPM, which is revolution per minute. To get the forcing frequencies in Hz (revolutions per second) just divide by 60. Once you have the forcing frequencies, pick the lower one and use the equations in the lesson to find the appropriate natural frequency and static deflection.

Eric